|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Приложение В**  **(обязательное)**  **Конфигурация оборудования**  **Конфигурация маршрутизатора**  Building configuration...  Current configuration : 5849 bytes  !  version 12.4  no service timestamps log datetime msec  no service timestamps debug datetime msec  no service password-encryption  !  hostname Router  !  !  !  enable secret 5 $1$mERr$5BePz5EP1ZeueutELQxCo.  !  !  !  ip dhcp pool Telephony  network 192.168.238.0 255.255.255.0  default-router 192.168.237.1  option 150 ip 192.168.237.1  !  !  !  ip cef  no ipv6 cef  !  !  !  !  !  !  !  !  !  !  ip ftp username Nikita  ip ftp password 1111  ip name-server 192.168.237.2  !  !  spanning-tree mode pvst  !  !  !  !  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| !  interface FastEthernet0/0  description LAN1  no ip address  duplex auto  speed 100  !  interface FastEthernet0/0.600  encapsulation dot1Q 600  ip address 192.168.230.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.601  encapsulation dot1Q 601  ip address 192.168.231.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.602  encapsulation dot1Q 602  ip address 192.168.236.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.603  encapsulation dot1Q 603  ip address 192.168.234.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.604  encapsulation dot1Q 604  ip address 192.168.233.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.605  encapsulation dot1Q 605  ip address 192.168.232.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.606  encapsulation dot1Q 606  ip address 192.168.235.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.607  encapsulation dot1Q 607  ip address 192.168.238.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.608  encapsulation dot1Q 608  ip address 192.168.239.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.609  encapsulation dot1Q 609 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ip address 192.168.237.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/0.610  encapsulation dot1Q 610  ip address 192.168.240.1 255.255.255.0  ip helper-address 192.168.237.2  !  interface FastEthernet0/1  no ip address  duplex auto  speed auto  shutdown  !  interface Vlan1  no ip address  shutdown  !  interface Vlan608  mac-address 0001.972b.ad01  no ip address  !  router rip  !  ip classless  !  ip flow-export version 9  !  !  !  !  !  !  !  telephony-service  max-ephones 29  max-dn 29  ip source-address 192.168.238.1 port 2000  auto assign 1 to 29  !  ephone-dn 1  number 100  !  ephone-dn 2  number 101  !  ephone-dn 3  number 102  !  ephone-dn 4  number 103  !  ephone-dn 5  number 104  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ephone-dn 6  number 105  !  ephone-dn 7  number 106  !  ephone-dn 8  number 107  !  ephone-dn 9  number 108  !  ephone-dn 10  number 109  !  ephone-dn 11  number 110  !  ephone-dn 12  number 111  !  ephone-dn 13  number 112  !  ephone-dn 14  number 113  !  ephone-dn 15  number 114  !  ephone-dn 16  number 115  !  ephone-dn 17  number 116  !  ephone-dn 18  number 117  !  ephone-dn 19  number 118  !  ephone-dn 20  number 119  !  ephone-dn 21  number 120  !  ephone-dn 22  number 121  !  ephone-dn 23  number 122  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ephone-dn 24  number 123  !  ephone-dn 25  number 124  !  ephone-dn 26  number 125  !  ephone-dn 27  number 126  !  ephone-dn 28  number 127  !  ephone-dn 29  number 128  !  ephone 1  device-security-mode none  mac-address 0001.4260.75AC  type 7960  button 1:1  !  ephone 2  device-security-mode none  mac-address 00E0.F9C0.3870  type 7960  button 1:2  !  ephone 3  device-security-mode none  mac-address 0001.C97C.6DEC  type 7960  button 1:3  !  ephone 4  device-security-mode none  mac-address 0030.A3EE.8E16  type 7960  button 1:4  !  ephone 5  device-security-mode none  mac-address 000A.F328.6BB9  type 7960  button 1:5  !  ephone 6  device-security-mode none  mac-address 0001.64A2.DD5A  type 7960  button 1:6  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ephone 7  device-security-mode none  mac-address 0002.1644.50AE  type 7960  button 1:7  !  ephone 8  device-security-mode none  mac-address 0090.2B81.23C5  type 7960  button 1:8  !  ephone 9  device-security-mode none  mac-address 0007.ECC4.8014  type 7960  button 1:9  !  ephone 10  device-security-mode none  mac-address 0090.2B26.4E36  type 7960  button 1:10  !  ephone 11  device-security-mode none  mac-address 00E0.A330.61AE  type 7960  button 1:11  !  ephone 12  device-security-mode none  mac-address 0001.C9D0.4ECC  type 7960  button 1:12  !  ephone 13  device-security-mode none  mac-address 0004.9A36.6AC0  type 7960  button 1:13  !  ephone 14  device-security-mode none  mac-address 00E0.B02C.E0C4  type 7960  button 1:14  !  ephone 15  device-security-mode none  mac-address 00E0.F75D.E4B9  type 7960  button 1:15  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ephone 16  device-security-mode none  mac-address 0060.3E98.E8A0  type 7960  button 1:16  !  ephone 17  device-security-mode none  mac-address 0006.2A8A.A993  type 7960  button 1:17  !  ephone 18  device-security-mode none  mac-address 0090.2B6E.76CD  type 7960  button 1:18  !  ephone 19  device-security-mode none  mac-address 000A.F3B0.E3EB  type 7960  button 1:19  !  ephone 20  device-security-mode none  mac-address 0006.2A16.7447  type 7960  button 1:20  !  ephone 21  device-security-mode none  mac-address 0003.E49B.7A4D  type 7960  button 1:21  !  ephone 22  device-security-mode none  mac-address 0002.16EE.3B84  type 7960  button 1:22  !  ephone 23  device-security-mode none  mac-address 0009.7CDD.0155  type 7960  button 1:23  !  ephone 24  device-security-mode none  mac-address 0002.166B.0801  type 7960  button 1:24  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ephone 25  device-security-mode none  mac-address 0002.1636.E511  type 7960  button 1:25  !  ephone 26  device-security-mode none  mac-address 0090.0C4D.D47D  type 7960  button 1:26  !  ephone 27  device-security-mode none  mac-address 000C.CF96.EBD6  type 7960  button 1:27  !  ephone 28  device-security-mode none  mac-address 000D.BDCB.09DA  type 7960  button 1:28  !  ephone 29  device-security-mode none  mac-address 0060.2F72.0C74  type 7960  button 1:29  !  line con 0  exec-timeout 5 0  password 10  login  !  line aux 0  !  line vty 0 4  login  !  !  !  end | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Конфигурация коммутатора Switch0**  Building configuration...  Current configuration : 4075 bytes  !  version 12.2  no service timestamps log datetime msec  no service timestamps debug datetime msec  no service password-encryption  !  hostname Switch  !  ip ftp username Nikita  ip ftp password 1111  enable secret 5 $1$mERr$5BePz5EP1ZeueutELQxCo.  !  !  !  ip host certificate.by 192.168.237.2  ip name-server 192.168.237.2  !  vtp domain sim  vtp mode transparent  !  !  spanning-tree mode pvst  spanning-tree extend system-id  !  vlan 600  name Useless  !  vlan 601  name Wireless  !  vlan 602  name Yellow  !  vlan 603  name lightBlue  !  vlan 604  name Blue  !  vlan 605  name Green  !  vlan 606  name Purple  !  vlan 607  name Bardo  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| vlan 608  name Admin  !  vlan 609  name Server  !  vlan 610  name Trunk  !  interface FastEthernet0/1  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/2  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/3  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/4  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/5  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/6  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/7  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/8  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/9  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| interface FastEthernet0/10  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/11  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/12  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/13  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/14  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/15  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/16  switchport access vlan 602  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/17  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/18  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/19  switchport trunk native vlan 610 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/20  switchport access vlan 601  switchport trunk native vlan 610  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/21  switchport access vlan 609  switchport trunk native vlan 8  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/22  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/23  switchport access vlan 601  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/24  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/1  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/2  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface Vlan1  no ip address  shutdown  !  interface Vlan608  mac-address 0060.7038.ad01  ip address 192.168.239.2 255.255.255.0  !  ip default-gateway 192.168.237.2  !  !  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| !  line con 0  password 10  login  exec-timeout 5 0  !  line vty 0 4  login  line vty 5 15  login  !  !  !  end | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Конфигурация коммутатора Switch1**  Building configuration...  Current configuration : 3898 bytes  !  version 12.2  no service timestamps log datetime msec  no service timestamps debug datetime msec  no service password-encryption  !  hostname Switch  !  ip ftp username Nikita  ip ftp password 1111  enable secret 5 $1$mERr$5BePz5EP1ZeueutELQxCo.  !  !  !  ip host certificate.by 192.168.237.2  ip name-server 192.168.237.2  !  vtp domain sim  vtp mode transparent  !  !  spanning-tree mode pvst  spanning-tree extend system-id  !  vlan 600  name Useless  !  vlan 601  name Wireless  !  vlan 602  name Yellow  !  vlan 603  name lightBlue  !  vlan 604  name Blue  !  vlan 605  name Green  !  vlan 606  name Purple  !  vlan 607  name Bardo  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| vlan 608  name Admin  !  vlan 609  name Server  !  vlan 610  name Trunk  !  interface FastEthernet0/1  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/2  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/3  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/4  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/5  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/6  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/7  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/8  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/9  switchport access vlan 600  switchport mode access | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/10  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/11  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/12  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/13  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/14  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/15  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/16  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/17  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/18  switchport access vlan 603  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/19  switchport access vlan 600  switchport mode access | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/20  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/21  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/22  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/23  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/24  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/1  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/2  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface Vlan1  no ip address  shutdown  !  interface Vlan608  description LAN1  mac-address 0000.0c12.0501  ip address 192.168.239.3 255.255.255.0  !  ip default-gateway 192.168.237.2  !  !  !  !  line con 0  password 10 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| login  exec-timeout 4 0  !  line vty 0 4  login  line vty 5 15  login  !  !  !  end | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Конфигурация коммутатора Switch2**  Building configuration...  Current configuration : 3805 bytes  !  version 12.2  no service timestamps log datetime msec  no service timestamps debug datetime msec  no service password-encryption  !  hostname Switch  !  ip ftp username Nikita  ip ftp password 1111  enable secret 5 $1$mERr$5BePz5EP1ZeueutELQxCo.  !  !  !  ip host certificate.by 192.168.237.2  ip name-server 192.168.237.2  !  vtp domain SIM  vtp mode transparent  !  !  spanning-tree mode pvst  spanning-tree extend system-id  !  vlan 600  name Useless  !  vlan 601  name Wireless  !  vlan 602  name Yellow  !  vlan 603  name lightBlue  !  vlan 604  name Blue  !  vlan 605  name Green  !  vlan 606  name Purple  !  vlan 607  name Bardo  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| vlan 608  name Admin  !  vlan 609  name Server  !  vlan 610  name Trunk  !  interface FastEthernet0/1  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/2  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/3  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/4  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/5  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/6  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/7  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/8  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/9  switchport access vlan 600  switchport mode access | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/10  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/11  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/12  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/13  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/14  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/15  switchport access vlan 600  switchport voice vlan 607  !  interface FastEthernet0/16  switchport access vlan 604  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/17  switchport access vlan 601  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/18  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/19  switchport access vlan 600  switchport mode access  switchport nonegotiate  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| interface FastEthernet0/20  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/21  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/22  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/23  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/24  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/1  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/2  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface Vlan1  no ip address  shutdown  !  interface Vlan608  mac-address 00d0.d3da.2301  ip address 192.168.239.4 255.255.255.0  !  ip default-gateway 192.168.237.2  !  !  !  !  line con 0  password 10  login  exec-timeout 5 0  !  line vty 0 4 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| login  line vty 5 15  login  !  !  !  end | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Конфигурация коммутатора Switch3**  Building configuration...  Current configuration : 3923 bytes  !  version 12.2  no service timestamps log datetime msec  no service timestamps debug datetime msec  no service password-encryption  !  hostname Switch  !  ip ftp username Nikita  ip ftp password 1111  enable secret 5 $1$mERr$5BePz5EP1ZeueutELQxCo.  !  !  !  ip host certificate.by 192.168.237.2  ip name-server 192.168.237.2  !  vtp domain sim  vtp mode transparent  !  !  spanning-tree mode pvst  spanning-tree extend system-id  !  vlan 600  name Useless  !  vlan 601  name Wireless  !  vlan 602  name Yellow  !  vlan 603  name lightBlue  !  vlan 604  name Blue  !  vlan 605  name Green  !  vlan 606  name Purple  !  vlan 607  name Bardo  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| vlan 608  name Admin  !  vlan 609  name Server  !  vlan 610  name Trunk  !  interface FastEthernet0/1  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/2  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/3  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/4  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/5  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/6  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/7  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/8  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/9  switchport access vlan 605 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| switchport mode access  switchport nonegotiate  !  interface FastEthernet0/10  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/11  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/12  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/13  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/14  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/15  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/16  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/17  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/18  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/19  switchport access vlan 600  switchport mode access  switchport nonegotiate  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| interface FastEthernet0/20  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/21  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/22  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/23  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface FastEthernet0/24  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface GigabitEthernet0/1  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface GigabitEthernet0/2  switchport access vlan 605  switchport mode access  switchport nonegotiate  !  interface Vlan1  no ip address  shutdown  !  interface Vlan608  mac-address 0007.ecc8.e401  ip address 192.168.239.5 255.255.255.0  !  ip default-gateway 192.168.237.2  !  !  !  !  line con 0  password 10 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| login  exec-timeout 5 0  !  line vty 0 4  login  line vty 5 15  login  !  !  !  end | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Конфигурация коммутатора Switch4**  Building configuration...  Current configuration : 3880 bytes  !  version 12.2  no service timestamps log datetime msec  no service timestamps debug datetime msec  no service password-encryption  !  hostname Switch  !  ip ftp username Nikita  ip ftp password 1111  enable secret 5 $1$mERr$5BePz5EP1ZeueutELQxCo.  !  !  !  ip host certificate.by 192.168.237.2  ip name-server 192.168.237.2  !  vtp domain sim  vtp mode transparent  !  !  spanning-tree mode pvst  spanning-tree extend system-id  !  vlan 600  name Useless  !  vlan 601  name Wireless  !  vlan 602  name Yellow  !  vlan 603  name lightBlue  !  vlan 604  name Blue  !  vlan 605  name Green  !  vlan 606  name Purple  !  vlan 607  name Bardo  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| vlan 608  name Admin  !  vlan 609  name Server  !  vlan 610  name Trunk  !  interface FastEthernet0/1  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/2  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/3  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/4  switchport access vlan 601  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/5  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/6  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/7  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/8  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/9  switchport access vlan 600  switchport mode access | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| switchport nonegotiate  !  interface FastEthernet0/10  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/11  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/12  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/13  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/14  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/15  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/16  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/17  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/18  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/19  switchport access vlan 606  switchport mode access  switchport nonegotiate  ! | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| interface FastEthernet0/20  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/21  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface FastEthernet0/22  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/23  switchport access vlan 606  switchport mode access  switchport nonegotiate  !  interface FastEthernet0/24  switchport access vlan 600  switchport mode access  switchport nonegotiate  switchport voice vlan 607  !  interface GigabitEthernet0/1  switchport trunk native vlan 610  switchport trunk allowed vlan 2-1005  switchport mode trunk  switchport nonegotiate  !  interface GigabitEthernet0/2  switchport access vlan 600  switchport mode access  switchport nonegotiate  !  interface Vlan1  no ip address  shutdown  !  interface Vlan608  mac-address 0001.6498.0601  ip address 192.168.239.6 255.255.255.0  !  ip default-gateway 192.168.237.1  !  !  !  !  line con 0  password 10 | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| login  exec-timeout 5 0  !  line vty 0 4  login  line vty 5 15  login  !  !  !  end | | | | | | |
|  |  |  |  |  | БГУИР 961401.011 | Лист |
|  |  |  |  |  | 90 |
| Изм | Лист | № докум. | Подп. | Дата |